**FAQ about ATF Network Account Activation**   
  
**Q: What is Phone Authorization?**A: Phone Authorization is a Service Offered by The ATF Network that will  
allow you to utilize more Repair Options for ALL SL3 Phones in the Market.  
Once a Phone is "Authorized", Super Dongle Repairs and SX-4 Authorization can be performed via Standalone Mode.  
  
  
**Q: Which Phones are supported?**A: All BB5 Phones are supported, but currently it only supports FBUS Connection.  
USB Connection "may" be supported in the future, but we still do not have a definite date for this to happen.  
  
  
**Q: Is the "Phone Authorization" Service Free?**A: No, it is not free. You need to purchase ATF Credits from your nearest  
ATF Reseller.   
You will first need to Create an ATF Network Account, then you can start using our Phone Authorization service for merely 5 Credits Per Phone. (5 credits is about 5 USD).  
  
  
  
**Q: So ALL phones need to be Authorized?**A: No, you ONLY NEED to Authorize the New BB5 Phones which have New HASHES that are NOT Supported by any other Team in the world. If your phone is using OLD HASH, then you can still work with it without paying for Authorization.  
  
  
**Q: How Many times do I need to Authorize the Phone?**A: You only need to Authorize the phone 1 time. Once it is authorized, you  
no longer need to perform authorization again.  
  
Can you repair Simlocks and IMEI from 100% erased SL3 and SIMLOC30 phones?  
No. We cannot repair or rebuild Simlocks for SL3 and SIMLOC30 phones. You can only repair these phones if you have a PM 120 Backup and an RPL Backup.  
  
  
**Q: Can I SD Repair and Authorize new SIMLOC30 phones?**A: YES. The ATF Network Supports ALL BB5 Phones in the Market.  
You just need to use FBUS Connection if you want to Authorize Phones.  
  
  
**Q: Which NEW HASHES are currently Supported by The ATF Network?**A: The ATF Network currently supported ALL 22 New HASHES released  
as of March 1, 2011.  
  
479C6DDE3942E12C429C1D6ADED803710E52EBD3  
C70CB07324056BC66A824347F40DB2D5E198D1B2  
916F75217F32081248B15C38DFC8E81B1803F26F  
25B977A055BE9B5DEC0C38A2A279C6958594B998  
7B045400E1752022F9EB80B0DEA9C65D6FBA5B05  
928E5FFB88D81E5F74729A212AB9D12EC755ED14  
2C05369F57CC3C4CF9E783E83D9B512B53E28D99  
3AB5DB70B45D23F1ADEEBB5734160706668138E1  
2B910DA4E0FBEFFFE5C65D3682854636C02881F7  
68597B9162BAB81AF74C56E78EA2588F2D968376  
EA81B32860B86EF4231A11831045F3E6AE071379  
8E309B54DA1ADDE27C2A035D63AACACDCB6C003B  
DA550B5BAAB517409088A3E4F3EB53AC9E57D0A3  
B8C3ADECFC997FCD8081D3DEAF870B8CBC33AE82  
B1A9CEADB5CE9CF9FB4F442150AA8E09D5F17F77  
46802B476C93A05CBAF76A64752086A9A7320E5C  
1B0D74C532CA1C6133940C740E8C786E49B99671  
700370BCF8AFBAB25DD62DBD124FD9CEEA461DFF  
87FAC992288DA497A663E5DDC0410B11521B8D0C  
55DF9CBCC80B17225043DDA1CC783C979BBCB7BC  
49A97E826B93BA20B7ED0B082475C0056EBB8F8D  
FEA0F9E21EF50B836924A9F25D85C643D8514505   
  
OLD HASHES are also supported, but you DO NOT NEED The ATF Network for OLD HASHES!!!  
  
  
**Q: Do I need Internet Connection to connect to the ATF Network?**A: Of course. But the good news is, after you have successfully   
Authorized your phone, you do not need the internet connection anymore  
to perform SD Repairs and SX4 Authorization. It will be Stand Alone.  
  
  
  
**Q: How long do I need to wait before my phone is Authorized?**A: Average time is 10 to 20 seconds, depending on your Internet Connection.  
  
  
**Q: Do you support the E7-00 which is the NEWEST BB5 Phone in the Marke**t?  
A: Yes, E7-00 HASH is supported by The ATF Network. However, you first need to find an FBUS Cable for E7-00 because The ATF Network DOES NOT SUPPORT USB Connection as of the moment.   
  
USB Connection will be supported in the future, but we cannot give you an actual date on when it will be released.